{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[[38,0,38,10],[43,0,43,10],[50,0,50,10],[76,0,76,10],[3,1,3,3],[3,4,3,10],[0,0,0,11],[1,0,1,3],[13,0,13,10],[24,0,24,10],[29,0,29,10]]}
[" ARK | 比较DELL工作站CPU产品"]
["2019/10/26 10:54:54"]
[null," 酷睿™ i7-9800X X"," 至强® W-2102 "," 至强® W-2123 "," 至强® 铜牌 3104 "," 至强® 铜牌 3204 "," 至强® 银牌 4210 "," 至强® 银牌 4110 "," Xeon金牌5118"," 至强® 金牌 6130 "," 至强® 铂金 8160 "]
["基本要素","DELL  T5820",null,null,"DELL T7920"]
["产品集"," 酷睿™ X 系列"," 至强® W "," 至强® W "," 至强","第二代至强","第二代 至强"," 至强"," 至强"," 至强"," 至强"]
["垂直市场","Desktop","Server","Server","Server","Server","Server","Server","Server","Server","Server"]
["编号","i7-9800X","W-2102","W-2123","3104","3204","4210","4110","5118","6130","8160"]
["状态","Launched","Launched","Launched","Launched","Launched","Launched","Launched","Launched","Launched","Launched"]
["发行日期","Q4'18","Q3'17","Q3'17","Q3'17","Q2'19","Q2'19","Q3'17","Q3'17","Q3'17","Q3'17"]
["光刻","14 nm","14 nm","14 nm","14 nm","14 nm","14 nm","14 nm","14 nm","14 nm","14 nm"]
["包括的项目","盒包无风扇"]
["使用条件",null,null,null,null,null,"Server/Enterprise","Server/Enterprise","Server/Enterprise","Server/Enterprise"]
["建议客户价格","$589.00 - $599.00","$202.00","$294.00","$213.00 - $223.00","$213.00 - $224.00","$501.00 - $511.00","$501.00 - $511.00","$1273.00","$1894.00 - $1900.00","$4702.00 - $4708.00"]
["性能"]
["内核数","8","4","4","6","6","10","8","12","16","24"]
["线程数","16","4","8","6","6","20","16","24","32","48"]
["基本频率","3.80 GHz","2.90 GHz","3.60 GHz","1.70 GHz","1.90 GHz","2.20 GHz","2.10 GHz","2.30 GHz","2.10 GHz","2.10 GHz"]
["最大睿频频率","4.40 GHz",null,"3.90 GHz",null,"1.90 GHz","3.20 GHz","3.00 GHz","3.20 GHz","3.70 GHz","3.70 GHz"]
["缓存","16.5 MB ","8.25 MB","8.25 MB","8.25 MB L3 Cache","8.25 MB","13.75 MB","11 MB L3 Cache","16.5 MB L3 Cache","22 MB L3 Cache","33 MB L3 Cache"]
["总线速度","8 GT/s","0 GT/s","0 GT/s"]
["QPI 链接数","0","0","0"]
[" 睿频加速 Max 技术 3.0 频率 ‡","4.50 GHz"]
["TDP","165 W","120 W","120 W","85 W","85 W","85 W","85 W","105 W","125 W","150 W"]
["UPI 链接数",null,"0","0","2","2","2","2","2","3","3"]
["补充信息"]
["提供嵌入式方案","否","否","否","否","否","是","是","是","是","否"]
["数据表","立即查看","立即查看","立即查看","立即查看",null,null,"立即查看","立即查看","立即查看","立即查看"]
["其他信息 URL",null,null,"立即查看","立即查看",null,null,"立即查看","立即查看","立即查看","立即查看"]
["产品简介",null,null,null,"立即查看",null,null,"立即查看","立即查看","立即查看","立即查看"]
["内存规格"]
["最大内存大小（取决于内存类型）","128 GB","512 GB","512 GB","768 GB","1 TB","1 TB","768 GB","768 GB","768 GB","768 GB"]
["内存类型","DDR4-2666","DDR4 1600/1866/2133/2400","DDR4 1600/1866/2133/2400/2666","DDR4-2133","DDR4-2133","DDR4-2400","DDR4-2400","DDR4-2400","DDR4-2666","DDR4-2666"]
["最大内存通道数","4","4","4","6","6","6","6","6","6","6"]
["ECC 内存支持 ‡","否","是","是","是","是","是","是","是","是","是"]
["最大内存带宽",null,"76.8 GB/s","85.3 GB/s"]
["物理地址扩展",null,"46-bit","46-bit"]
["最大内存速度",null,null,null,"2133 MHz","2133 MHz","2400 MHz","2400 MHz","2400 MHz","2666 MHz","2666 MHz"]
[" 傲腾™ DC 永久性内存支持",null,null,null,null,"否","否"]
["扩展选项"]
["可扩展性","1S Only","1S Only","1S Only","2S","2S","2S","2S","4S","S4S","S8S"]
["PCI Express 修订版","3.0","3.0","3.0","3.0","3.0","3.0","3.0","3.0","3.0","3.0"]
["PCI Express 通道数的最大值","44","48","48","48","48","48","48","48","48","48"]
["PCI Express 配置 ‡",null,"x4, x8, x16","x4, x8, x16"]
["封装规格"]
["支持的插槽","FCLGA2066","FCLGA2066","FCLGA2066","FCLGA3647","FCLGA3647","FCLGA3647","FCLGA3647","FCLGA3647","FCLGA3647","FCLGA3647"]
["最大 CPU 配置","1","1","1"]
["散热解决方案规范","PCG 2017X"]
["TJUNCTION","95°C"]
["TCASE",null,"66","65","78°C","77°C","78°C","77°C","81°C","87°C","85°C"]
["封装大小",null,"45mm x 52.5mm","45mm x 52.5mm","76.0mm x 56.5mm","76.0mm x 56.5mm","76.0mm x 56.5mm","76.0mm x 56.5mm","76.0mm x 56.5mm","76.0mm x 56.5mm","76.0mm x 56.5mm"]
["先进技术"]
[" 傲腾™ 内存支持 ‡","是","否","否","否",null,null,"否","否","否","否"]
[" 睿频加速 Max 技术 3.0 ‡","是","否","否","否","否","否","否","否","否","否"]
[" 睿频加速技术 ‡","2.0","否","2.0","否","否","2.0","2.0","2.0","2.0","2.0"]
[" 超线程技术 ‡","是","否","是","否","否","是","是","是","是","是"]
[" 虚拟化技术 ‡","是","是","是","是","是","是","是","是","是","是"]
[" 定向 I/O 虚拟化技术 ‡","是","是","是","是","是","是","是","是","是","是"]
[" 64 ‡","是","是","是","是","是","是","是","是","是","是"]
["指令集扩展","Intel® SSE4.1, Intel® SSE4.2, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512","Intel® SSE4.2, Intel® AVX, Intel® AVX2, Intel® AVX-512"]
["AVX-512 FMA 单元数","2","1","2","1","1","1","1","1","2","2"]
["增强型英特尔 SpeedStep® 技术","是","是","是","是","是","是","是","是","是","是"]
[" Speed Shift Technology",null,"是","是","是","是","是","是","是","是","是"]
[" 博锐™ 平台资格‡",null,"是","是","是","是","是","是","是","是","是"]
["有扩展页表 (EPT) 的 VT-x ‡",null,"是","是","是","是","是","是","是","是","是"]
[" Transactional Synchronization Extensions – New Instructions ( TSX-NI)",null,"是","是","是","是","是","是","是","是","是"]
["指令集",null,"64-bit","64-bit"]
["空闲状态",null,"是","是"]
[" 按需配电技术",null,"是","是"]
["温度监视技术",null,"是","是"]
[" Flex Memory Access",null,"否","否"]
[" 身份保护技术 ‡",null,"是","是"]
[" Volume Management Device (VMD)",null,"是","是","是","是","是","是","是","是","是"]
[" 深度学习提升",null,null,null,null,"是","是"]
[" Speed Select 技术——性能配置",null,null,null,null,"否","否"]
[" Speed Select 技术——基本频率",null,null,null,null,"否","否"]
[" 资源导向技术",null,null,null,null,"是","是"]
["安全性与可靠性"]
[" AES 新指令：","是","是","是","是","是","是","是","是","是","是"]
["执行禁用位 ‡","是","是","是","是","是","是","是","是","是","是"]
["安全密钥",null,"是","是"]
[" Software Guard Extensions",null,"否","否"]
[" 内存保护扩展",null,"是","是"]
[" 操作系统守护",null,"是","是"]
[" Trusted Execution Technology（ 可信执行技术） ‡",null,"是","是","是","是","是","是","是","是","是"]
[" Boot Guard",null,"是","是"]
["基于模式的执行控制 (MBE)",null,null,null,"是","是","是","是","是","是","是"]
[" 确保运行技术",null,null,null,null,"否","否",null,"是","是","是"]